(module SofleKeyboard-footprint:LED (layer F.Cu) (tedit 5D8F83FF)
  (fp_text reference J1 (at 0 -2.54 -180) (layer F.SilkS) hide)
  (fp_text value LED (at 0 7.62 -180) (layer F.Fab) hide)
  (fp_text user VCC (at -2.2 0.1 -180) (layer B.SilkS))
  (fp_text user VCC (at -2.2 0.1 -180) (layer B.SilkS))
  (fp_text user GND (at -2.1 5.1 -180) (layer B.SilkS))
  (fp_text user LED (at -2.2 2.5 -180) (layer B.SilkS))
  (fp_text user LED (at -2.2 2.5 -180) (layer B.SilkS))
  (fp_text user GND (at -2.1 5.14 -180) (layer F.SilkS))
  (pad 3 thru_hole rect (at 0 5.1) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole rect (at 0 2.5) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0 90) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask))
)
