(module SofleKeyboard-footprint:MJ-4PP-9 (layer F.Cu) (tedit 5D8BAE3B)
  (fp_text reference J2 (at -0.889 6.4135) (layer F.Fab))
  (fp_text value 4PIN (at 0 14) (layer F.Fab) hide)
  (fp_text user TRRS (at -0.75 6.45) (layer F.SilkS))
  (fp_text user TRRS (at -0.75 6.45) (layer F.SilkS))
  (pad 4 thru_hole oval (at -2.1 11.8) (size 1.7 2.5) (drill oval 1 1.5) (layers *.Cu *.Mask F.SilkS)
    (clearance 0.15))
  (pad 1 thru_hole oval (at 2.1 10.3) (size 1.7 2.5) (drill oval 1 1.5) (layers *.Cu *.Mask F.SilkS)
    (clearance 0.15))
  (pad 2 thru_hole oval (at 2.1 6.3) (size 1.7 2.5) (drill oval 1 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole oval (at 2.1 3.3) (size 1.7 2.5) (drill oval 1 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 8.5) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 0 1.5) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole oval (at -3.85 6.3) (size 1.7 2.5) (drill oval 1 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole oval (at -3.85 3.3) (size 1.7 2.5) (drill oval 1 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole oval (at 0.35 11.8) (size 1.7 2.5) (drill oval 1 1.5) (layers *.Cu *.Mask F.SilkS)
    (clearance 0.15))
  (pad 1 thru_hole oval (at -3.85 10.3) (size 1.7 2.5) (drill oval 1 1.5) (layers *.Cu *.Mask F.SilkS)
    (clearance 0.15))
  (pad "" np_thru_hole circle (at -1.75 1.5) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at -1.75 8.5) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (model "../../../../../../Users/pluis/Documents/Magic Briefcase/Documents/KiCad/3d/AB2_TRS_3p5MM_PTH.wrl"
    (at (xyz 0 0 0))
    (scale (xyz 0.42 0.42 0.42))
    (rotate (xyz 0 0 90))
  )
)
