(module SofleKeyboard-footprint:RotaryEncoder_Alps_EC11E-Switch_Vertical_H20mm-keebio_modified (layer F.Cu) (tedit 5D5C0C22)
  (descr "Alps rotary encoder, EC12E... with switch, vertical shaft, http://www.alps.com/prod/info/E/HTML/Encoder/Incremental/EC11/EC11E15204A3.html")
  (tags "rotary encoder")
  (fp_text reference SW25 (at 4.24 4.6) (layer F.SilkS) hide)
  (fp_text value Rotary_Encoder_Switch (at 0 7.9) (layer F.Fab))
  (pad A thru_hole circle (at -7.5 -2.5) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad C thru_hole circle (at -7.5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad B thru_hole circle (at -7.5 2.5) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad MP thru_hole rect (at 0 -5.6) (size 3.2 2) (drill oval 2.8 1.5) (layers *.Cu *.Mask))
  (pad MP thru_hole rect (at 0 5.6) (size 3.2 2) (drill oval 2.8 1.5) (layers *.Cu *.Mask))
  (pad S2 thru_hole circle (at 7 -2.5) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad S1 thru_hole circle (at 7 2.5) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Rotary_Encoder.3dshapes/RotaryEncoder_Alps_EC11E-Switch_Vertical_H20mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
